IAC-19-B5.2.10

**Robust Forest Classification using Hyperspectral Imaging, Laser Scanning and Satellite Imagery**

**Vasilii Mosin a\*, Roberto Aguilar a, Alexander Platonov a, Albert Vasiliev b, Alexander Kedrov b, and Anton Ivanov a**

a Space Center, Skolkovo Institute of Science and Technology, Moscow, Russian Federation, vasilii.mosin@skoltech.ru

b Perm State University, Perm, Perm Krai, Russian Federation,

\* Corresponding Author

**Abstract**

Wood products are an important export for Russia. Understanding the status of trees and their classification is an ongoing task for many organizations. Currently, documentation of forests is done manually and there is a number of initiatives to implement automatic forest classification. A particular case described in the present paper showcases how aerial survey data supplements satellite imagery in order to achieve higher classification accuracy of forest tree species. Moreover, applicability of different data types, such as LiDAR, RGB, and hyperspectral (NIR and VIS) for the task at hand is investigated.

In the paper, we present the experiment to use hyperspectral forest classification (using a UAV), which is then used in the context of satellite imagery, airborne laser scanning, and manual identification. We actively employ machine learning algorithms for classification and recognition tasks.

The project began with an expedition to the northern region of Arkhangelsk (Russia) in August 2018. The main goals of the expedition were data acquisition with the help of UAVs (one RGB and one hyperspectral), as well as observing various weather conditions and their effect on the data collected.

Validation of the results was performed in four separate polygons, where in-situ data was collected by manually recording tree locations and species. In this project we evaluated the precision of trees identification from UAV hyperspectral data, helped by ALS and high-resolution satellite imagery (50 cm).

Supervised machine learning algorithms, namely Support Vector Machine (SVM) and Random Forest (RF), were applied and evaluated for automatic tree species classification task. Preliminary exploratory data analysis using unsupervised techniques was also done and described. An object-based classification has been performed by delineating individual tree crowns beforehand with the help of LiDAR data. Various hyperspectral features have been identified for use in classification algorithms complemented by on-ground spectroscopic benchmark data.

In this paper, we prove applicability of the proposed method and workflow in real life application. Results validation was done using data from the observation parcels, where trees were manually labeled. The next step is design of a system with finely tuned filters, which will make possible robust species classification at a cost much lower than hyperspectral imaging. We aim at classification accuracy of 90% that will allow for change proposal for current forestry policy and legislature to enable the use of UAVs in forestry for classification purposes.

**Keywords:** hyperspectral imagery, LiDAR data, machine learning, forest inventory, tree species, tree detection

**Acronyms/Abbreviations**

ALS Airborne LiDAR System

CHM Canopy Height Model

DBH Diameter at Breast Height

DTM Digital Terrain Model

DSM Digital Surface Model

LIDAR Light Detection and Ranging

NDVI Normalized Difference Vegetation Index

NIR Near Infrared

RF Random Forest

RGB Red, Green, Blue

SVM Support Vector Machines

UAV Unmanned Aerial Vehicle

1. **Introduction**

Forest inventory plays an important role in terms of economical and environmental sustainability both regionally and globally. It is especially relevant in case of Russia, since its territories cover around 20% of world’s forest reserves.1 In accordance with the current forestry legislation in Russia, forest inventory shall be done manually, which is time consuming and expensive. In this project, an attempt to build an automatic trees detection and classification technology, based on remote sensing and machine learning is presented and tested. In order to allow a widespread use of this technology in the industry for forest inventory, classification accuracy of 95% shall be achieved. A combination of machine learning and remote sensing has demonstrated a big potential for solving different tasks in such areas as precision agriculture, land cover changes detection, urban environment monitoring, maritime navigation and control, etc. Additionally, it has application in forest classification, a particular case of land cover classification. In general, any land cover classification task can be categorized either as pixel-based or as object-based, but the latter usually shows better results.2–4 Moreover, in forestry applications object-based trees species classification is more valuable, since it gives more detailed information about a forest structure. There are two approaches for object-based forest classification: classification at the individual tree level, classifying every tree separately, or area-based classification, when dominant tree species are predicted for different areas of a forest. In this work, the case of individual tree level forest species classification is considered, because forestry legislation requires to have information for each tree rather than general statistics for whole parcels of a forest. Nowadays, hyperspectral data has become extensively used in different land cover classification tasks, as it contains more information than multispectral imagery and, therefore, allows to catch subtle differences in akin materials. For example, Utsav et al.5have described different remote sensing scenarios, in which a high number of spectral bands is important. Also, Kang et al.6have presented a performance comparison of different algorithms applied on hyperspectral imagery for land cover classification, providing a benchmark data. Moreover, there are various deep learning approaches for hyperspectral data processing.7–9 Furthermore, current research on forest classification is based on hyperspectral imaging. Existing investigations describe different approaches based on using different instruments and algorithms classifying different tree species in different regions. For instance, Support Vectors Machine (SVM) algorithm was applied on hyperspectral imagery with 160 bands (410-990 nm) to classify 3 groups of trees (Spruces, Pines, and Deciduous trees) in Norway and the accuracy of 92% was achieved.1089% classification accuracy was obtained when classifying 13tree species (8 Deciduous and 5 Coniferous) in Austria using the same hyperspectral imaging, as in the previous example, but with Random Forest (RF) classifier.11 Nevalainen et al.12have managed to achieve 95% accuracy for tree species classification in Finland. They classified 4 tree species (Spruce, Birch, Pine, and Larch) by RF algorithm using hyperspectral imagery with spectral resolution of 33 channels (500-900 nm). The approach for trees detection and classification presented in this work consists of two steps. In the beginning, individual trees are detected using LiDAR data.

Then, detected trees are classified by their hyperspectral properties using machine learning classifiers. Aiming to compare results of airborne technologies with technical characteristics of cheaper and more scalable one, the same experiment was performed using space-borne technology, in this case, using a sub metric multispectral sensor. Section 2 surveys methods and algorithms used for trees detection and classification in this project as well as an expedition for collection of LiDAR, hyperspectral and reference trees data together with instruments characteristics and data pre-processing procedures. Section 3 contains results of the experiments done in this project and description of evaluation schemes and performance metrics. Sections 4 and 5 are devoted to discussion of the results and conclusions accordingly.

*1.1 Subsection headings*

Subsection headings are in *italics* and placed flush on the left hand margin of the column.

*1.1.1 Sub-subsection headings*

Sub-subsection headings are in *italics* and placed flush on the left hand margin of the column.

**2. Data and Methodology**

A special expedition to Arkhangelsk region (northern Russia) was performed in August 2018 for data collection purposes. Experimental area belongs to Krasnoborsky district forestry division (Figure 1).




Figure 1. Geographic location of Arkhangelsk region with the highlighted area (red rectangle) corresponding to Krasnoborsky district at 61◦28′N 45◦34′E

This territory is covered by plain cultivated boreal forests. Four test polygons with a size of 150 m by 200 m each were selected for experimental data collection.




Figure 2. Location of the four experimental polygons, each of them with an area 0.03 Km2

Detailed descriptions of the data collection procedures, instruments characteristics, as well as pre-processing steps for LiDAR, airborne hyperspectral, spaceborne multispectral, and reference trees data are given in Sections~\ref{sec:lidar}, \ref{sec:hyperspectral}, and \ref{sec:reference} respectively. Individual Tree Crowns (ITCs) detection strategy is described in Section~\ref{sec:detection}. Section~\ref{sec:classification} is devoted to tree species classification procedure.

*2.1 Airborne Laser Scanning*

Canopy Height Model (CHM) enables the analysis of trees height and crowns area. It is obtained by calculating the difference between the Digital Surface Model (DSM) and Digital Terrain Model (DTM). In our case, it was derived from a point cloud sampled using airborne laser scanning (ALS) LiDAR sensor Leica ALS70, onboard a manned aircraft. The overall result of mapping was a 5 points/m2 density point cloud.

As first step, raw point cloud was pre-processed with Terrasolid software. This software takes LiDAR raw data, and outputs a file in *las* format, which contains position and classification of every point based on ASPRS Standard \cite{ASPRS}. For later steps, a pipeline to automatically generate the CHM was developed, taking as input a *las* file, and producing a raster.

In order to generate the DTM, all points classified as *ground* were selected. As the density of points in this classification was only 0.5 points / m2, the rasterization was performed using a linear interpolation method with a resolution of 1 m by 1 m.

As for the DSM calculation, all points classified as *high vegetation* were processed. For the rasterization, cell size of the grid is a key parameter, an appropriate cell size will help to avoid raster gaps and preserve sufficient details. Grid cell size was obtained from $c = \sqrt{1/n}$, where $c$ is grid cell size, and $n$ is the density of points~\cite{WU201682}, that in this area was 6.3 points / m2, obtaining a 0.4 m grid cell size. Per each cell, the highest point within its area was selected (Figure \ref{fig:dsm}).




Figure 3. Process of DSM rasterization, from a point cloud gathered from ALS, by selecting points with highest value per each square. Per each cell of 0.16 m2in the grid, the highest point in the vector is selected, and its height value is assigned to the raster.

Finally, CHM in raster format was calculated with the operation *CHM = DSM - DTM*, having the same DSM resolution of 0.16 m2. After generating the raster, data noise or errors may still exist in the CHM. A first attempt of filtering using Gaussian smoothing was performed as described by Wu et al.~\cite{WU201682}, but due to the low density of points, the top and mean height of trees was considerably decreasing, up to 30\%. For this reason, another approach was followed, instead grey dilation was used for filtering. As shown in Figure 4, it improved the persistence of canopy height, since it only enlarges bright regions (tree crowns), and without altering the height of the top of the trees.




Figure 4. Comparison of results between Gaussian smoothing and grey dilation for resulting CHM filtering in the same region, with an area of 625 m2

*2.2 Airborne Hyperspectral Imagery*

For hyperspectral data collection, a OXI VNIR-40 hyperspectral camera from Gamaya company, mounted on a fixed-wing drone Geoscan-101 was used. The camera has 16 bands in visible range (450-670 nm) and 25 bands in near-infrared range (600-900 nm). The flights were done in early afternoon when the sun was at a maximum elevation angle, in order to minimize shadowing effects. The flights were performed at the constant altitude of 250 m with the speed of 60 Km/h. The spatial resolution of hyperspectral sensor was set to 5.5 cm/pixel.

Hyperspectral imagery pre-processing included optical and radiometric calibration. On ground spectroscopy measurements were acquired during each flight and it was used as a calibration information to transform raw pixel values into reflectance values. However, changing weather conditions (sunny and cloudy) during the flights have resulted in significant brightness differences in hyperspectral values along the same flight, and between flights. Nevertheless, these effects were partially mitigated by normalization procedure applied when performing tree species classification. Optically and radiometrically calibrated images were then stitched together into orthophotoplans. Afterwards, bad quality spectral bands were removed and the resulting dimensionality of hyperspectral cubes was reduced to 32 (15 VIS and 17 NIR) spectral bands and 10 cm ground resolution.

Due to low geolocation accuracy, additional georeferencing procedure using ground control points (GCPs) was applied to collocate LiDAR and hyperspectral imagery. CHM rasters computed from LiDAR point clouds served as a base layer for this georeferencing procedure. For each test site, between the 5 and 7 most recognizable tree tops were found on both CHM rasters and hyperspectral cubes and used as GCPs.



 

Figure 5. Examples of true color composites from airborne hyperspectral imagery (left) and spaceborne multispectral imagery (right) for the same area.

*2.3 Satellite-based Multispectral Imagery*

*2.4 Reference data*

For every polygon described in Figure 2, there is a sub polygon, 100 m by 50 m size that contains annotations of the four main tree species presented in test region: *Spruce, Birch, Fir, and Pine*. All trees with diameter at breast height (DBH) larger than 6 cm were labeled, 3000 trees in total. Table 1 contains the amount of different reference tree species for every test polygon.




Figure 6. Example of the test polygon (red dot on the left map) with true color composite obtained from hyperspectral imagery (Red: 622 nm, Green: 578 nm, Blue: 461 nm) and the labeled reference trees location.

Table 1. Distribution of reference trees by class in every polygon

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Polygon | Spruce | Birch | Fir | Pine | Total |
| pp1 | 603 | 224 | 20 | - | 847 |
| pp2 | 464 | 322 | 89 | - | 875 |
| pp3 | 210 | 98 | - | 227 | 535 |
| pp4 | 528 | 153 | 7 | - | 688 |
| Total | 1805 | 797 | 116 | 227 | 2945 |

One of the issues with the labelling process on field was that there was no information about the tree height. Moreover, trees were labeled regardless their visibility from above. For this reason, non-visible trees from remote optical sensors were filtered out. Heights of the labeled trees were estimated using regression models based on DBH values and heights information for some of the model trees in the test polygons. Locations of remaining trees were adjusted visually in QGIS software using CHM rasters and true color composites from hyperspectral imagery for exact matching their positioning with the corresponding tree crowns. Table 2 presents the final numbers of the reference trees collected.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Polygon | Spruce | Birch | Fir | Pine | Total |
| pp1 | - | - | - | - | - |
| pp2 | 424 | 181 | 41 | - | 471 |
| pp3 | 66 | 43 | - | 139 | 248 |
| pp4 | 231 | 19 | 3 | - | 327 |
| Total | 539 | 324 | 41 | 39 | 1046 |

Unfortunately, it was not possible to co-locate most of the reference trees with the hyperspectral imagery in the first test polygon, thus it was decided to exclude all the labeled trees in this polygon from further analysis completely.

*2.4 Individual Tree Crowns Detection*

Individual tree crowns detection (ITCd) is a preliminary step for object-based tree species classification. Most of the existing methods for ITCd are based on local maximum (LM) filtering applied either on CHM rasters obtained from LiDAR data~\cite{Popescu, Popescu2, Tiede} or on high spatial resolution imagery~\cite{WULDER2000103, TIDA, Pouliot, NOVOTNY}. The results are more stable when using LiDAR data, since LM points correspond to the real tree crown tops in this case. While in the case of using imagery for ITCd, LM points may actually be just the brightness peaks and not the real tree crown tops. Moreover, it was shown that detection accuracy using imagery is more or less comparable with detection accuracy using LiDAR data only if imagery resolution is high (around 5-15 cm) and for lower resolution imagery (less than 30 cm) detection accuracy is significantly lower\cite{Pouliot}. There is another approach for ITCd using deep learning~\cite{cnn, cascade\_nn}, but it requires a considerable amount of training data.

In this work, the following approach for ITCd was used. Firstly, non-vegetation areas, such as roads, dead trees, etc., were excluded by masking out Normalized Difference Vegetation Index (NDVI) raster using threshold value of 0.6. NDVI is calculated for every pixel according to:

where NDVI - pixel's NDVI value, NIR - pixel's value in near-infrared range, RED - pixel's value in red range.

After, low vegetation areas, with value lower than 10 m on CHM, were masked out. Therefore, only the areas containing high vegetation are left for further analysis. Finally, for these areas ITCs were detected on CHM rasters using the approach based on LM filtering described by Popescu et al.~\cite{Popescu}.

*2.5 Tree Species Classification*

There are two approaches for classification tasks in remote sensing as it was discussed in Section~\ref{sec:introduction}. The first one is pixel-based classification when each pixel is classified separately. This approach is usually applied with coarse resolution imagery, for instance field crop classification using 30 m resolution Landsat 8 satellite. In the other hand, object-based classification is performed using the information about the whole object, for either individual crowns, or areas. In general, it was shown that object-based approach is more stable and outperforms pixel-based approach in most cases; for this reason, object-based tree species classification is used along this work.

First of all, boundaries of the classified objects shall be defined to be able to extract features inside these regions. Tree crowns delineation methods are usually applied for segmentation of exact shapes of the crowns, and can follow different approaches, including point clouds obtained from LiDAR~\cite{Popescu, Popescu2, Tiede}, and some others methods just relying on the image brightness values in the absence of structural information~\cite{TIDA, NOVOTNY, Pouliot}. However, in case of high resolution imagery, it is enough to use more simple strategies to define object boundaries, as, for example, Nevalainen et al.~\cite{Nevalainen2017IndividualTD} extracted features for tree species classification inside a circle area around detected tree top.

Based on (our own paper if published next week), a 1 m fixed radius circle provides the best accuracy results for classification in cross validation. For both hyperspectral airborne and multispectral satellite imagery, boundaries were defined using this technique as shown in Figure 7.




Figure 7. Examples of differences in amount of extracted pixels of tree crowns in hyperspectral airborne and multispectral satellite data during features calculation step due to different imagery resolutions

There exist several strategies to construct feature vectors for classification from hyperspectral data. For example, Nevalainen et al.~\cite{Nevalainen2017IndividualTD} used mean, median, and some of their threshold values as features. In this project, it was decided to use only mean values per each spectral band as features, since there is one-to-one correspondence between features and spectral bands in this case and, therefore, the results will be more interpretable and it is possible to estimate the importance of the spectral bands for tree species classification. The number of extracted features for hyperspectral airborne data is 32, which is the total number of bands in hyperspectral imagery used in this project. Additionally, normalization is applied in order to reduce the effects of brightness differences in hyperspectral imagery as well as the shadowing effects. Moreover, normalization improves the overall accuracy of hyperspectral imagery classification, which was demonstrated by Cao et al.~\cite{normalization} where it is recommended to use normalization per spectral bands, but in this project normalization per pixel values is applied, since it gives better results in case of changing weather conditions during the flights. The exact formula for normalization used in this project is the following:

Where - the value of the pixel in the spectral band , - the total number of bands and - normalized value of the pixel in the spectral band . Figure 8 shows mean normalized spectral values averaged from hyperspectral airborne data per tree species for the reference trees in different test polygons.




Figure 8. Mean (normalized) spectral values of the reference trees for four tree species in different test polygons using hyperspectral airborne imagery.

In terms of the multispectral satellite data, 8 features were extracted, following the same normalization process as for hyperspectral imagery. Figure 9 shows mean normalized spectral values averaged from multispectral satellite data per tree species for the reference trees in different test polygons.




Figure 9. Mean (normalized) spectral values of the reference trees for four tree species in different test polygons using multispectral satellite imagery.

**3. Results**

Performance of the classification algorithms is estimated using leave-one-out cross-validation (LOOCV) scheme, which is a special case of cross-validation when each sample is used for validation exactly one time. The following two metrics are calculated in order to compare the algorithms: Overall Accuracy (OA) (Eq.~\ref{eq:accuracy}) -- the proportion of correctly classified samples and F-score (Eq.~\ref{eq:f\_score}) -- harmonic mean of precision (Eq.~\ref{eq:precision}) and recall (Eq.~\ref{eq:recall}).

where *N* -- the total number of samples, *TP* -- the number of true positive classifications, *FP* -- the number of false positive classifications, *FN* -- the number of false negative classifications.

Table~\ref{tab:cv} contains *OA* and *F-score* values for different classifiers on cross-validation when using different crown area sizes for features extraction. The most optimal circle radius value for tree species classification is 1.0 m according to the experiments in this work. Additionally, confusion matrices for all classifiers are built when using 1.0 m circle radius area (Figure~\ref{fig:confusion}), in order to show how each tree species of the reference trees are classified during cross-validation.



**4. Results**

Results should be clear and concise.

**5. Discussion**

This should explore the significance of the results of the work, not repeat them. A combined Results and Discussion section is often appropriate. Avoid extensive citations and discussion of published literature.

**6. Conclusions**

The main conclusions of the study may be presented in a short Conclusions section, which may stand alone or form a subsection of a Discussion or Results and Discussion section.

**Acknowledgements**

This section is not numbered.

**Appendix A (Title)**

This section is not numbered.

**Appendix B (Title)**

This section is not numbered.

**Etc.**

**References**

In the text

Indicate references by number(s) in square brackets in line with the text. The actual authors can be referred to, but the reference number(s) must always be given.

Example: “..... as demonstrated [3,6]. Barnaby and Jones [8] obtained a different result ....”

List of references

Number the references (numbers in square brackets) in the list in the order in which they appear in the text.

Examples:   
Reference to a journal publication:

[1] J. van der Geer, J.A.J. Hanraads, R.A. Lupton, The art of writing a scientific article, J. Sci. Commun. 163 (2010) 51–59.

Reference to a conference/congress paper:

[2] Y.-W. Chang, J.-S. Chern, Ups and Downs of Space Tourism Development in 60 Years from Moon Register to SpaceShipTwo Crash, **IAC-15-E4.2.8, 66th International Astronautical Congress, Jerusalem, Israel, 2015, 12 – 16 October.**

Reference to a book:

[3] W. Strunk Jr., E.B. White, The Elements of Style, fourth ed., Longman, New York, 2000.

Reference to a chapter in an edited book:

[4] G.R. Mettam, L.B. Adams, How to prepare an electronic version of your article, in: B.S. Jones, R.Z. Smith (Eds.), Introduction to the Electronic Age, E-Publishing Inc., New York, 2009, pp. 281–304.

Reference to a website:

[5] E. Mack, Could Virgin Galactic’s Spaceport America be put up for sale? 23 February 2015, <http://www.gizmag.com/spaceport-america-hits-nags/36200/>, (accessed 30.04.16).

1] “World bank open data.”

https://data.worldbank.org(2016). (Accessed: 12 August 2019).[2] Whiteside, T. G., Boggs, G. S., and Maier, S. W., “Comparing object-based and pixel-based classificationsfor mapping savannas,”International Journal of Applied Earth Observation and Geoinformation13(6), 884– 893 (2011).[3] C Weih, R. and D Riggan, N., “Object-based classification vs. pixel-based classification: Comparitive im-portance of multi-resolution imagery,”International Archives of the Photogrammetry, Remote Sensing andSpatial Information Sciences - ISPRS Archives38(01 2010).[4] Juniati, E. and N. Arrofiqoh, E., “Comparison of pixel-based and object-based classification using parametersand non-parameters approach for the pattern consistency of multi scale landcover,”ISPRS - InternationalArchives of the Photogrammetry, Remote Sensing and Spatial Information SciencesXLII-2/W7, 765–771(09 2017).[5] Gewali, U. B., Monteiro, S. T., and Saber, E., “Machine learning based hyperspectral image analysis: Asurvey,”ArXivabs/1802.08701(2018).[6] Kang, X., Li, S., and Benediktsson, J. A., “Hyperspectral image classification: A benchmark,” in [2017IEEE International Geoscience and Remote Sensing Symposium (IGARSS)], 3632–3639 (July 2017).[7] Li, Y., Xie, W., and Li, H., “Hyperspectral image reconstruction by deep convolutional neural network forclassification,”Pattern Recognition63, 371 – 383 (2017).[8] Lee, H. and Kwon, H., “Going deeper with contextual cnn for hyperspectral image classification,”IEEETransactions on Image Processing26, 4843–4855 (Oct 2017).[9] Zhang, M., Li, W., and Du, Q., “Diverse region-based cnn for hyperspectral image classification,”IEEETransactions on Image Processing27, 2623–2634 (June 2018).[10] Dalponte, M., rka, H. O., Ene, L. T., Gobakken, T., and Nsset, E., “Tree crown delineation and tree speciesclassification in boreal forests using hyperspectral and als data,”Remote Sensing of Environment140, 306– 317 (2014).[11] Maschler, J., Atzberger, C., and Immitzer, M., “Individual tree crown segmentation and classification of 13tree species using airborne hyperspectral data,”Remote Sensing10(8) (2018).[12] Nevalainen, O., Honkavaara, E., Tuominen, S., Viljanen, N., Hakala, T., Yu, X., Hyypp ̈a, J., Saari, H.,P ̈ol ̈onen, I., Imai, N. N., and Tommaselli, A. M. G., “Individual tree detection and classification withuav-based photogrammetric point clouds and hyperspectral imaging,”Remote Sensing9, 185 (2017).[13] The Imaging & Geospatial Information Society, “LAS SPECIFICATION,” (08 2011).[14] Wu, B., Yu, B., Wu, Q., Huang, Y., Chen, Z., and Wu, J., “Individual tree crown delineation using localizedcontour tree method and airborne lidar data in coniferous forests,”International Journal of Applied EarthObservation and Geoinformation52, 82 – 94 (2016).[15] Popescu, S., Wynne, R., and Nelson, R., “Estimating plot-level tree heights with lidar: local filtering with acanopy-height based variable window size,”Computers and Electronics in Agriculture37, 71–95 (12 2002).[16] Popescu, S. and Wynne, R., “Seeing the trees in the forest: Using lidar and multispectral data fusionwith local filtering and variable window size for estimating tree height,”Photogrammetric Engineering andRemote Sensing70, 589–604 (05 2004).[17] Tiede, D., “A full gis-based workflow for tree identification and tree crown delineation using laser scanning.,”International Archives of Photogrammetry, Remote Sensing and Spatial Information SciencesXXXVI, 9 –14 (01 2005).[18] Wulder, M., Niemann, K., and Goodenough, D., “Local maximum filtering for the extraction of tree locationsand basal area from high spatial resolution imagery,”Remote Sensing of Environment73, 103–114 (07 2000).[19] S Culvenor, D., “Tida: An algorithm for the delineation of tree crowns in high spatial resolution remotelysensed imagery,”Computers & Geosciences - COMPUT GEOSCI28, 33–44 (02 2002).[20] Pouliot, D., King, D., Bell, F. W., and Pitt, D., “Automated tree crown detection and delineation in high-resolution digital camera imagery of coniferous forest regeneration,”Remote Sensing of Environment82,322–334 (10 2002).[21] Novotn ́y, J., “Individual tree crowns delineation using local maxima approach and seeded region growingtechnique,” (2011).

[22] Li, W., Fu, H., Yu, L., and Cracknell, A. P., “Deep learning based oil palm tree detection and counting forhigh-resolution remote sensing images,”Remote Sensing9, 22 (2016).[23] Tianyang, D., Jian, Z., Sibin, G., Ying, S., and Jing, F., “Single-tree detection in high-resolution remote-sensing images based on a cascade neural network,”ISPRS International Journal of Geo-Information7,367 (09 2018).[24] Cao, F., Yang, Z., Ren, J., Jiang, M., and Ling, W., “Does normalization methods play a role for hyper-spectral image classification?,”CoRRabs/1710.02939(2017).[25] Pedregosa, F., Varoquaux, G., Gramfort, A., Michel, V., Thirion, B., Grisel, O., Blondel, M., Prettenhofer,P., Weiss, R., Dubourg, V., Vanderplas, J., Passos, A., Cournapeau, D., Brucher, M., Perrot, M., andDuchesnay, E., “Scikit-learn: Machine learning in Python,”Journal of Machine Learning Research12,2825–2830 (2011)